**Provo City Energy Department** Sheet No. 1-2

**PROVO CITY ENERGY DEPARTMENT**

**ELECTRIC SERVICE SCHEDULE NO. 6**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**General Service -- High Voltage**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**AVAILABILITY**

This schedule is available at any point on the Energy Department electric system where facilities

of adequate capacity and standard high voltage levels are available.

**APPLICATION**

To qualify for service under this rate schedule, a customer must (1) have immediate access

(proximity) to the Energy Department’s high voltage electric system; (2) accept delivery at

Provo’s standard high voltage levels; (3) accept delivery at a substation that is dedicated solely

to the customer’s use and (4) own the substation at the point of delivery.

**CHARACTER OF SERVICE**

This schedule is for alternating current, three-phase service supplied at approximately 46,000

volts or greater, through a single point of delivery. Standby or resale service is not permitted.

**MONTHLY RATE**

The monthly billing for electric service, excluding charges for other utility services and taxes,

shall be the sum of the following charges:

**Customer Service Charge:** $227.82 per Service Connection

**Demand Charge:** $14.79 per kW

**Energy Charge:** $0.0368 per kWh

**DEMAND METERING**

The kW billing demand shall be the highest measured 15-minute kW for the billing period,

adjusted for power factor as specified in this schedule.

**Provo City Energy Department** Sheet No. 2-2

**ELECTRIC SERVICE SCHEDULE No. 6** (Continued)

**POWER FACTOR**

The Energy Department may, at its option, install metering equipment to allow the utility to

determine the reactive components of power utilized by the customer. The customer’s utilization

of equipment shall not result in a power factor at the point of delivery of less than 95% lagging

at the time of maximum demand. Should the power factor be less than 95% lagging during any

month, the Energy Department may adjust the readings taken to determine the billed demand by

multiplying the kW obtained through such readings by 95% and by dividing the result by the

power factor actually established at the time of maximum demand during the current month.

Such adjusted readings shall be used in determining the billing demand.

The Energy Department reserves the right, at its option, to utilize kVA meters, kVAR meters,

and / or other appropriate meters in those metering installations where the customer’s power

factor is believed to be unsatisfactory on a continuous basis according to the Energy

Department’s standards. If such meters are installed, the billing demand in kW or kVA may be

computed from such instruments.

**MINIMUM CHARGE**

The minimum monthly charge shall be the Customer Charge listed above under the Monthly

Rate section.

**TAX ADJUSTMENTS**

The amount computed at the above Monthly Rate shall be subject to taxes, assessments and

surcharges imposed by Provo City or any governmental authority authorized to levy said taxes,

assessments or surcharges.

**TERMS AND CONDITIONS**

Service under this schedule will be in accordance with the Energy Department’s electric service

standards and policies and terms and conditions set forth by the Department’s standard

application requirements and Provo City Ordinances, including any future additions or

amendments.